#!/usr/bin/env bash
#
# Build tests for BigTreeTech GTR 1.0
#

# exit on first failure
set -e

restore_configs
opt_set MOTHERBOARD BOARD_BTT_GTR_V1_0 SERIAL_PORT 3 \
        EXTRUDERS 8 TEMP_SENSOR_1 1 TEMP_SENSOR_2 1 TEMP_SENSOR_3 1 TEMP_SENSOR_4 1 TEMP_SENSOR_5 1 TEMP_SENSOR_6 1 TEMP_SENSOR_7 1
opt_enable SDSUPPORT USB_FLASH_DRIVE_SUPPORT USE_OTG_USB_HOST \
           REPRAP_DISCOUNT_FULL_GRAPHIC_SMART_CONTROLLER BLTOUCH LCD_BED_TRAMMING BED_TRAMMING_USE_PROBE \
           NEOPIXEL_LED Z_SAFE_HOMING FILAMENT_RUNOUT_SENSOR NOZZLE_PARK_FEATURE ADVANCED_PAUSE_FEATURE
# Not necessary to enable auto-fan for all extruders to hit problematic code paths
opt_set E0_AUTO_FAN_PIN PC10 E1_AUTO_FAN_PIN PC11 E2_AUTO_FAN_PIN PC12 NEOPIXEL_PIN PF13 \
        X_DRIVER_TYPE TMC2208 Y_DRIVER_TYPE TMC2130 \
        FIL_RUNOUT_PIN 3 FIL_RUNOUT2_PIN 4 FIL_RUNOUT3_PIN 5 FIL_RUNOUT4_PIN 6 FIL_RUNOUT5_PIN 7 FIL_RUNOUT6_PIN 8 FIL_RUNOUT7_PIN 9 FIL_RUNOUT8_PIN 10 \
        FIL_RUNOUT4_STATE HIGH FIL_RUNOUT8_STATE HIGH
opt_enable FIL_RUNOUT4_PULLUP FIL_RUNOUT8_PULLUP
exec_test $1 $2 "GTT GTR | OTG USB Flash Drive | 8 Extruders | Auto-Fan | Mixed TMC Drivers | Runout Sensors (distinct)" "$3"

# clean up
restore_configs
